Installation and building image procedure

Step 1: Install the Broadcom BCM963xx release.

# sudo su
# mkdir /tmp/consumer
# cd /tmp/consumer
copy bcm963xx_3.10L.02_consumer_release.tar to /tmp/consumer
# tar xvfz bcm963xx_3.10L.02_consumer_release.tar
# ./consumer_install

Step 2: Build the desired image.
# cd /opt/bcm963xx_router
# make PROFILE=WMVN25E2plus_ST

Image file is located in /opt/bcm963xx_router/images
